IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A-MSDU section | | | | |
| Date: 2011-07-18 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Simone Merlin | Qualcomm Inc | 5775 Morehouse Dr  San Diego, CA 92109 | 8588451243 | smerlin@gmail.com |

Abstract

This document provides resolution for the comments listed below

Comments are from: 11-11-0907-0x-00ac-lb178-comments-tgac-d1-0.xlsx

Comments refer to: Draft P802.11ac\_D1.0.pdf

**Comments**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 2292 | 75.32 | 9.11 | ambiguous reference - | change "its" to "the recipient's" | AGREE IN PRINCIPLE | MAC |
| 2293 | 75.43 | 9.11 | ambiguous reference - whose capability element? | change "element" to "element of the recipient" | AGREE IN PRINCIPLE | MAC |
| 3060 | 75.44 | 9.11 | Is A-MSDU support mandatory for 'Single MPDU'?. 11n states "Support for the reception of an A-MSDU, where the A-MSDU is carried in a QoS data MPDU with Ack Policy (#10128)equal to Normal Ack and the A-MSDU is not aggregated within an A-MPDU, is andatory for an HT STA" | change to: "Support for the reception of an A-MSDU, where the A-MSDU is carried in a QoS data MPDU with Ack Policy (#10128)equal to Normal Ack and the A-MSDU is not aggregated within an A-MPDU or is sent as part of a Single MPDU frame, is mandatory for an HT STA" | AGREE IN PRINCIPLE | MAC |
| 3063 | 75.28 | 9.11 | specify to which capability the sentence is referred to: "A STA shall not transmit an A-MSDU in a HT PPDU to a STA that exceeds its maximum A-MSDU length capability." | A STA shall not transmit an A-MSDU in a HT PPDU to a STA that exceeds its maximum A-MSDU length capability, indicated in the HT Capability element | AGREE IN PRINCIPLE | MAC |

**Discussion**

Added the reference to the Capabilities element most recently received from the recipient STA.

Added a sentence clarifying that reception of an A-MSDU is mandatory for a VHT STA in case it is carried in a VHT Single MPDU

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3349 | 75.28 | 9.11 |  |  | What happens if a VHT STA wants to retransmit an A-MSDU previously sent in a VHT PPDU using an HT PPDU, but this A-MSDU exceeds the max A-MSDU size? | Clarify | AGREE IN PRINCIPLE | MAC |

**Discussion**

In that case the A-MSDU cannot be transmitted; this limitation is already present in the text though the description of the maximum supported A-MSDU and MPDU lengths; A NOTE is added to further clarify

Instructions to the Editor

**9.11 A-MSDU operation**

***Modify the section as follows:***

***L36 P75 of 11acD1.0***

A STA shall not transmit an A-MSDU in a HT PPDU to a STA that exceeds the maximum A-MSDU length

indicated in the Maximum A-MSDU Length field of the most recent HT Capabilities Info field sent by the recipient STA.

A VHT STA that sets the Maximum MPDU Length in the VHT Capabilities element to indicate 3895 octets

shall set the Maximum A-MSDU Length in the HT Capabilities element to indicate 3839 octets. A VHT STA

that sets the Maximum MPDU Length in the VHT Capabilities element to indicate 7991 octets or 11 454 octets

shall set the Maximum A-MSDU Length in the HT Capabilities element to indicate 7935 octets.

A STA shall not transmit an MPDU in a VHT format PPDU to a STA that exceeds the maximum MPDU

length capability indicated in the most recent VHT Capability element sent by the recipient STA.

NOTE—An A-MSDU that meets the A-MSDU length limit for transmission in a VHT PPDU may exceed the A-MSDU length limit for an HT PPDU and thus not be retransmitted in an HT PPDU

***Modify the paragraph starting at PAG 803 L9***

Support for the reception of an A-MSDU, where the A-MSDU is carried in a QoS data MPDU with Ack Policy

(#10128)equal to Normal Ack is mandatory in the following cases:

-- for an HT STA if the A-MSDU is not aggregated within an A-MPDU,

-- for a VHT STA if the A-MSDU is sent in a VHT Single MPDU.