IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolutions to Miscellaneous MAC Comments  |
| Date: Sep 15, 2011 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Chunhui (Allan) Zhu | Samsung Electronics |  | +1-408-544-2751 | c.zhu@samsung.com |
|  |  |  |  |  |

Abstract

This document provides resolutions to misc MAC comments. The following CIDs are covered in this document.

* **Sub-Clause 8.2.4.1.8:** 3696, 2325
* **Sub-Clause 9.19.2.2:** 3806
* **Sub-Clause 9.22.5.3 (in 11mb):** 3079
* **Sub-Clause 9.24:** 3568
* **Sub-Clause 10.8.3:** 2580, 3337, 3439, 3581

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 3696 | 20.06 | 6 | 8.2.4.1.8 | The added text for the More Data field is coming after sentence: "The More Data field is set to 0 in all other directed frames." The added text does not fit to More Data field explanations. | Please correct the clause and make the 802.11ac addition compatible with the existing base text.  | **Agree in Principle** The text of this paragraph describes an exception of the “all other directed frames”. Need to change the existing base text.See the resolution in 11-11/1194. |
| 2325 | 21.08 | 8 | 8.2.4.1.8 | Is this signalling between the VHT AP and a single VHT STA (in individually addressed frames)? If so, clarify the usage (individualy addressed, and frame types), and why is the last sentence of this paragraph plural? If this is for group addressed frames, the prerequisitie for the non-AP STAs being VHT capable needs to be clarified - must all STAs in the BSS be VHT? | Clarify this paragraph's intended usage scenarios, and detail the pre-requisites. | **Agree in Principle** The description of this paragraph is not clear. This is the signalling between the VHT AP and a single VHT STA. It is not for group addressed frames.See the resolution in 11-11/1194. |

**Discussion:**

The description of the More Data field for the TXOP PS purpose is not integrated into the existing text gracefully. For example, in the general description of the field, the first paragraph of this subclause, it says,

“The More Data field is 1 bit in length and is used to indicate to a STA in PS mode that more BUs are buffered for that STA at the AP. The More Data field is valid in directed data or management type frames transmitted by an AP to a STA in PS mode. A value of 1 indicates that at least one additional buffered BU is present for the same STA.”

This description does not cover the case of TXOP PS mode, in which the STAs are running in Active mode. In addition, this is the signalling between the VHT AP and a single VHT STA. So the placement of this added paragraph should be relocated to before the description of the group addressed frames.

**TGac editor: insert the following new paragraph in REVmb D8.0 at P412, L32, before the sentence “The More Data field is set to 0 in all other directed frames.” as follows**

In a VHT BSS, the More Data field may be used to indicate a power save operation only meaningful within a TXOP, where STAs are running in active mode. In this case, this field is set to 1 in frames transmitted by VHT AP to indicate that it has more frames to transmit to a non-AP STA.

**TGac editor: Delete the paragraphs in D1.0, P21, L3-L9**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 3806 | 79.48 | 48 | 9.19.2.2 | "associated with secondary ACs (secondary ACs)" What does this mean? | Clarify or fix this notation. | **Agree in Principle**Some editorial errors exist in this paragraph.See the resolution in 11-11/1194. |

**TGac editor: modify D1.0 P79, L46-L48, as follows**

The sharing of the EDCA TXOP occurs when an EDCAF associated with the primary AC has obtained access to the medium and shares access with EDCAFs associated with secondary ACs during MU PPDU transmission.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 3079 | 85.43 |  | 9.22.5.3 | 9.22.5.3 L-SIG TXOP protection rules at the TXOP responder. Clarify that an VHT STA shall not use this mode.  |  | **Agree in Principle**A VHT STA should not use L-SIG TXOP protection.See the resolution in 11-11/1194. |

**Discussion:**

This can be resolved by setting VHT STA’s L-SIG TXOP Protection Support field in the HT Capability element to zero so a VHT STA will never use the L-SIG TXOP protection.

**TGac editor: modify D1.0 P85, L43, as follows**

 ***Insert the following sub-clause title.***

**9.22.5.3 L-SIG TXOP protection rules at the TXOP responder**

***Insert the following sentence at the end of this sub-clause.***

A VHT STA shall always set the L-SIG TXOP Protection Support field to zero during association and re-association.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 3568 | 85.54 | 54 | 9.24 | The definition of non-A-MPDU frame includes VHT single MPDU, so "It is a non-A-MPDU frame or a VHT single MPDU," is a tautology. | Remove the phrase "or a VHT single MPDU" when applied to non-A-MPDU frame. | **Agree**See the resolution in 11-11/1194. |

**TGac editor: modify D1.0 P85, L54, as follows**

— It is a non-A-MPDU frame and

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 3581 | 95.17 | 17 | 10.8.3 | "Any local maximum transmit power received in the combination of a VHT Transmit Power Envelopeelement and an Extended Power Constraint element from the AP in its BSS or another STA inits IBSS and"Is there an MBSS case to cover too? | Make any necessary statement about MBSS. | **Disagree**The paragraph is origined in the baseline document, not from 11ac. It is within TGmb’s work scope to update the baseline text. In addition, a MBSS is a BSS. |
| 3439 | 95.35 | 35 | 10.8.3 | Local Maximum Transmit Power is per BSS and does not provide means to control power per STA (according to its link budget and QoS requirements) for the purpose of interference reduction. Suggest to add TPC per STA that would apply to its uplink (STA to AP) transmissions | Details will be provided in TG meeting | DisagreeIn the absence of any details, this comment is rejected. |
| 3337 | 95.46 | 46 | 10.8.3 | Either? Hm, so a VHT STA is not required to use a VHT TPE IE and EPC IE? And if it does, it is required to not use an HT PC IE? | Clarify | **Agree in Principle**.The requirements are not clear and should be clarified.See the resolution in 11-11/1194. |
| 2580 | 95.47 | 47 | 10.8.3 | For VHT the Transmit Power Envelope element is replacing the Country element. Won't applications in regulated domains require the Country element? | Add the Transmit Power Envelope element as a third member of the combination, instead of a replacement to the Country element. | **Agree in Principle**.The Country element should be in the combination.See the resolution in 11-11/1194. |

**Discussion:**

This paragraph has two problems.

1. It makes possible that a VHT AP/STA is not required to use the the combination of a VHT Transmit Power Envelope element and an Extended Power Constraint element. Instead, a VHT AP/STA is allowed to use the combination of a Country element and a Power Constraint element only, which I believe is not our intent.
2. Country element is removed from the combination for the VHT combination, which I think we should add it back.

Sugguest separating the descriptions for VHT and non-VHT cases.

**TGac editor: modify D1.0 P95, L42-L49, as follows**

An AP in a BSS and a STA in an IBSS shall advertise the regulatory maximum transmit power for that

STA’s operating channel in Beacon frames and Probe Response frames using a Country element. A non-VHT AP in a BSS and a non-VHT STA in an IBSS shall advertise the local maximum transmit power for that STA’s operating channel in Beacon frames and Probe Response frames using the combination of a Country element and a Power Constraint element. A VHT AP in a BSS and a VHT STA in an IBSS shall advertise the local maximum transmit power for that STA’s operating channel in Beacon frames and Probe Response frames using the combination of a Country element, a Power Constraint element, a VHT Transmit Power Envelope element and an Extended Power Constraint element.