IEEE P802.11
Wireless LANs

|  |
| --- |
| Max Number of MSDUs in an A-MSDU |
| Date: 2012-03-08 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Simone Merlin | Qualcomm Inc | 5775 Morehouse DrSan Diego, CA 92109 | 8588451243 | smerlin@qualcomm.com |
| Guido Frederiks | Qualcomm Inc |  |  |  |
| Shukla Ashish | Qualcomm Inc |  |  |  |
| Menzo Wentink | Qualcomm Inc |  |  |  |

Abstract

Comment is from: 11-12-0752-03-00ac-lb188-comment-tgac-d3-0.xls

Comment and editorial instructions refer to: Draft P802.11ac\_D3.0.pdf

# Comment

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 6855 | 116.15 | 9.11 | There is no limit on the number of MSDUs that can be packed in an A-MSDU sent in a MPDU. Potentially the number of MSDUs can be very large. As an example, assuming small packets of 62Bytes (e.g. ~TCP ACK) an MPDU of 11454Bytes could include up to 184 MSDUs. For a max sized A-MPDU of 64 MPDUs this can potentially result in >11000 MSDUs. These numbers are exemplary to illustrate the problem. In general, processing a high and unpredictable number of MSDUs increases complexity of receiver | Add an optional indication for a receiver VHT STA to signal to a transmitter VHT STA that the number of MSDUs per MPDU shall be less than a given number; ability to limit the number of MSDUs in a MPDU to <= 16 is suggested. The indication can be in the form of a capability indication (TBD). The current operation mode (no limit) is also preserved; Restriction can only be signaled by a VHT STA to a VHT STA; restriction refers to number of MSDUs sent in any MPDU where A-MSDU is allowed. | REVISE. Adopt resolution as in DCN 12/0917r1 (this document) |

# Discussion

In the current specifications (D3.0 and 802.11-2012) there is no limit on the number of MSDUs that can be packed in an A-MSDU sent in a MPDU. Potentially the number of MSDUs can be very large. As an example, assuming small packets of 62Bytes (TCP Ack)



an MPDU of 11454Bytes could include up to 183 MSDUs.

Even worse, a rogue (but spec compliant) STA may send MPDUs with QoS control AMSDU set to 1, and rest of payload set to all 0s, which could be interpreted as series of 14bytes MSDUs (DA==SA==length all 0). In this case a 11454Byte MPDU may include up to 11454/14 = 818 MSDUs!

In general, the processing of a high and unpredictable number of MSDUs within a single MPDU implies increased complexity of receiver design. Note that in a MPDU there is only one FCS field at the end, which determines the correctness of all the MSDUs included in the MPDU; being the FCS at the end, by the time an error is detected a huge number of MSDUs may have been already processed, uselessly. The design though needs to account for the worst case, hence the increased memory requirement and processing complexity.

If we further consider that up to 64MPDUs can be aggregated, a PPDU could end up carrying thousands of MSDUs. Receiver design need also to take into account this total unpredictable number.

# Proposed resolution:

Add an optional indication for a receiver VHT STA to signal to a transmitter VHT STA that the number of MSDUs per A-MSDU (i.e. per MPDU) shall be less than a given number.

The limit refers to A-MSDUs sent within any type of PPDU/frame where A-MSDU is allowed.

Transmitters have to honor the limitation indicated by the receiving STA.

The preferred limitation can be indicated by one of the reserved bits of the VHT Capabilities Info field, such as B30.

The limitation can be defined as

* + B30=0 🡪 no limitations
	+ B30=1🡪 any A-MSDU shall carry no more than X MSDUs.
		- [where we can define X to be e.g. 16 ]

Note that the proposed limit is optional so that STAs that do not want to limit the number of A-MSDUs are free to preserve the operation with no limitations

Limiting the A-MSDU number to e.g. 16 has no or limited impact on the throughput.

In fact assuming typical MSDUs of 1500Bytes, a limit of e.g. 16 MSDUs per MPDU would already exceed the maximum MSDU size of 11454; in this case there is no impact to throughput.

For e.g. MSDUs of 500 Bytes, the limit of 16 MSDUs would result in ~8000Bytes A-MSDU i.e. it would not cause any throughput loss up to the maximum MPDUs size of 7991 Bytes, and it may cause some loss in case of max MPDU size of 11454 Bytes.

**Editorial instructions**

**9.11 A-MSDU operation**

***Add the following paragraph at the end of the section***

A VHT STA shall not transmit an A-MSDU that includes more than X MSDUs to a recipient VHT STA, if the Max Number of MSDUs in A-MSDU field is set to 1 in the VHT Capabilities Info field from the recipient STA.

***Replace Figure 8-401bs with the following one***

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | B0 B1 | B2 B3 | B4 | B5 | B6 | B7 | B8 B10 | B11 | B12 | B13 B15 |
|  | Maximum MPDU Length | Supported Channel Width Set | Rx LDPC | Short GI for 80 MHz | Short GI for 160 and 80+80 MHz | Tx STBC | Rx STBC | SU Beamformer Capable | SU Beamformee Capable | Compressed Steering Number of Beamformer Antennas Supported |
| Bits: | 2 | 2 | 1 | 1 | 1 | 1 | 3 | 1 | 1 | 3 |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| B16 B18 | B19 | B20 | B21 | B22 | B23 B25 | B26 B27 | B28 | B29 | B30 B31 |
| Number Of Sounding Dimensions | MU Beamformer Capable | MU Beamformee Capable | VHT TXOP PS | +HTC-VHT Capable | Maximum A-MPDU Length Exponent | VHT Link Adaptation Capable | Rx Antenna Pattern Consistency | Tx Antenna Pattern Consistency | Max Number of MSDUs in A-MSDU | Reserved |
| 3 | 1 | 1 | 1 | 1 | 3 | 2 | 1 | 1 | 1 | 1 |
| * VHT Capabilities Info field
 |

**Append to Table 8-183u the following row**

|  |  |  |
| --- | --- | --- |
| Max Number of MSDUs in A-MSDU | Indicates the maximum number of MSDUs in a A-MSDU the STA is able to receive | If set to 1, the STA supports reception of at most X MSDUs in each A-MSDU. Set to 0 if the STA is not indicating a maximum supported number of MSDUs in a A-MSDU. |