IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11ak PICS | | | | |
| Date: 2014-11-02 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Donald Eastlake | Huawei Technologies | 155 Beaver Street, Milford, MA 01757 USA | +1-508-333-2270 | d3e3e3@gmail.com |
|  |  |  |  |  |

Abstract

This document proposes initial PICS for 802.11ak to resolve CC17 CID 76.

# Introduction

This document proposes initial PICS for 802.11ak to resolve CC17 CID 76.

### B.4.3 IUT configuration

***Add the following entry renumbering the existing CF31 to be CF32:***

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | |  |  |  |  |  |  |  | |  | Item | IUT configuration | References | Status | Support |  | |  | CF31 | GLK STA | 10.45 (GLK BSS Operation) | O | Yes **◻**︎ No ◻ |  | |  |  |  |  |  |  |  | |  |  |  |  |  |  |

#### B.4.4.2 MAC frames

***Add the following entries:***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  | Item | MAC frame | References | Status | Support |  |
|  | FT43 | LPD Data | 5.1.4 (MSDU format) | M | Yes **◻**︎ No ◻ |  |
|  | FT44 | EPD Data | 5.1.4 (MSDU format), 10.46 (EPD Operation) | O | Yes **◻**︎ No ◻ |  |
|  | FR44 | LPD Data | 5.1.4 (MSDU format) | M | Yes **◻**︎ No ◻ |  |
|  | FR45 | EPD Data | 5.1.4 (MSDU format), 10.46 (EPD Operation) | O | Yes **◻**︎ No ◻ |  |
|  |  |  |  |  |  |  |

#### B.4.4.4 MAC addressing functions

***Add the folliwng entries:***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  | Item | MAC Address function | References | Status | Support |  |
|  | AD12 | Receive Type 0 SYNRA | 9.42 (SYNRA address filtering operation) | CF31:M | Yes **◻**︎ No ◻ |  |
|  | AD13 | Send Type 0 SYNRA | 9.42 (SYNRA address filtering operation) | CF31:O | Yes **◻**︎ No ◻ N/A ◻ |  |
|  | AD14 | Receive Type 1 and 2 SYNRA | 9.42 (SYNRA address filtering operation) | CF31:O | Yes **◻**︎ No ◻ N/A ◻ |  |
|  | AD15 | Send Type 1 and 2 SYNRA | 9.42 (SYNRA address filtering operation) | CF31:O | Yes **◻**︎ No ◻ N/A ◻ |  |
|  |  |  |  |  |  |  |