P802.11
Wireless LANs

|  |
| --- |
| TGaq –Pre-association Service Discovery Protocol |
| Date: 2014-03-14 |
| Author(s): |
| Name | Company | Address | Phone | email |
| SK Yong | Apple | 3 Infinte Loop, Cupertino, CA |  | skyong [at] apple.com |
| Chris Hartman | Apple |  |  |  |
| Yong Liu | Apple |  |  |  |
| Eric Wong | Apple |  |  |  |
| Pradboth Varshney | Nokia |  |  |  |
| James Yee | MediaTek |  |  |  |
| Chao Chun Wang | MediaTek |  |  |  |
| Jing-Rong Hsieh | HTC |  |  |  |
| Cheol Ryu  | ETRI |  |  |  |
| Carolyn Heide | Ruckus Wireless |  |  |  |
| Santosh Abraham | Qualcomm |  |  |  |
| George Cherian | Qualcomm |  |  |  |
| Rob Slater | Motorola Mobility |  |  |  |

Abstract

This document describes the Pre-association Service Discovery protocol

P802.11aq™/D0.02
Draft Trial-Use Standard for for Information technology--Telecommunications and information exchange between systems Local and metropolitan area networks--Specific requirements Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications – Amendment: Pre-Association Discovery

Sponsor

Wireless LAN Working Group (C/LM/WG802.11)

of the

IEEE Computer Society/LAN/MAN Standards Committee (C/LM)

Approved <Date Approved>

IEEE-SA Standards Board

Copyright © 2014 by The Institute of Electrical and Electronics Engineers, Inc.

Three Park Avenue

New York, New York 10016-5997, USA

All rights reserved.

This document is an unapproved draft of a proposed IEEE Standard. As such, this document is subject to change. USE AT YOUR OWN RISK! IEEE copyright statements SHALL NOT BE REMOVED from draft or approved IEEE standards, or modified in any way. Because this is an unapproved draft, this document must not be utilized for any conformance/compliance purposes. Permission is hereby granted for officers from each IEEE Standards Working Group or Committee to reproduce the draft document developed by that Working Group for purposes of international standardization consideration. IEEE Standards Department must be informed of the submission for consideration prior to any reproduction for international standardization consideration (stds.ipr@ieee.org). Prior to adoption of this document, in whole or in part, by another standards development organization, permission must first be obtained from the IEEE Standards Department (stds.ipr@ieee.org). When requesting permission, IEEE Standards Department will require a copy of the standard development organization's document highlighting the use of IEEE content. Other entities seeking permission to reproduce this document, in whole or in part, must also obtain permission from the IEEE Standards Department.

IEEE Standards Department

445 Hoes Lane

Piscataway, NJ 08854, USA

Abstract: This amendment defines modifications to the IEEE 802.11 standard, above the physical layer (PHY), to enable delivery of pre-association Service Discovery information by IEEE 802.11 stations (STAs).

Keywords: <Select this text and type or paste keywords>

[[1]](#footnote-1)•

Important Notices and Disclaimers Concerning IEEE Standards Documents

IEEE documents are made available for use subject to important notices and legal disclaimers. These notices and disclaimers, or a reference to this page, appear in all standards and may be found under the heading “Important Notice” or “Important Notices and Disclaimers Concerning IEEE Standards Documents.”

**Notice and Disclaimer of Liability Concerning the Use of IEEE Standards Documents**

IEEE Standards documents (standards, recommended practices, and guides), both full-use and trial-use, are developed within IEEE Societies and the Standards Coordinating Committees of the IEEE Standards Association (“IEEE-SA”) Standards Board. IEEE (“the Institute”) develops its standards through a consensus development process, approved by the American National Standards Institute (“ANSI”), which brings together volunteers representing varied viewpoints and interests to achieve the final product. Volunteers are not necessarily members of the Institute and participate without compensation from IEEE. While IEEE administers the process and establishes rules to promote fairness in the consensus development process, IEEE does not independently evaluate, test, or verify the accuracy of any of the information or the soundness of any judgments contained in its standards.

IEEE does not warrant or represent the accuracy or content of the material contained in its standards, and expressly disclaims all warranties (express, implied and statutory) not included in this or any other document relating to the standard, including, but not limited to, the warranties of: merchantability; fitness for a particular purpose; non-infringement; and quality, accuracy, effectiveness, currency, or completeness of material. In addition, IEEE disclaims any and all conditions relating to: results; and workmanlike effort. IEEE standards documents are supplied “AS IS” and “WITH ALL FAULTS.”

Use of an IEEE standard is wholly voluntary. The existence of an IEEE standard does not imply that there are no other ways to produce, test, measure, purchase, market, or provide other goods and services related to the scope of the IEEE standard. Furthermore, the viewpoint expressed at the time a standard is approved and issued is subject to change brought about through developments in the state of the art and comments received from users of the standard.

In publishing and making its standards available, IEEE is not suggesting or rendering professional or other services for, or on behalf of, any person or entity nor is IEEE undertaking to perform any duty owed by any other person or entity to another. Any person utilizing any IEEE Standards document, should rely upon his or her own independent judgment in the exercise of reasonable care in any given circumstances or, as appropriate, seek the advice of a competent professional in determining the appropriateness of a given IEEE standard.

IN NO EVENT SHALL IEEE BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO: PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE PUBLICATION, USE OF, OR RELIANCE UPON ANY STANDARD, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE AND REGARDLESS OF WHETHER SUCH DAMAGE WAS FORESEEABLE.

**Translations**

The IEEE consensus development process involves the review of documents in English only. In the event that an IEEE standard is translated, only the English version published by IEEE should be considered the approved IEEE standard.

**Official statements**

A statement, written or oral, that is not processed in accordance with the IEEE-SA Standards Board Operations Manual shall not be considered or inferred to be the official position of IEEE or any of its committees and shall not be considered to be, or be relied upon as, a formal position of IEEE. At lectures, symposia, seminars, or educational courses, an individual presenting information on IEEE standards shall make it clear that his or her views should be considered the personal views of that individual rather than the formal position of IEEE.

**Comments on standards**

Comments for revision of IEEE Standards documents are welcome from any interested party, regardless of membership affiliation with IEEE. However, IEEE does not provide consulting information or advice pertaining to IEEE Standards documents. Suggestions for changes in documents should be in the form of a proposed change of text, together with appropriate supporting comments. Since IEEE standards represent a consensus of concerned interests, it is important that any responses to comments and questions also receive the concurrence of a balance of interests. For this reason, IEEE and the members of its societies and Standards Coordinating Committees are not able to provide an instant response to comments or questions except in those cases where the matter has previously been addressed. For the same reason, IEEE does not respond to interpretation requests. Any person who would like to participate in revisions to an IEEE standard is welcome to join the relevant IEEE working group.

Comments on standards should be submitted to the following address:

 Secretary, IEEE**-**SA Standards Board

 445 Hoes Lane

 Piscataway, NJ 08854 USA

**Laws and regulations**

Users of IEEE Standards documents should consult all applicable laws and regulations. Compliance with the provisions of any IEEE Standards document does not imply compliance to any applicable regulatory requirements. Implementers of the standard are responsible for observing or referring to the applicable regulatory requirements. IEEE does not, by the publication of its standards, intend to urge action that is not in compliance with applicable laws, and these documents may not be construed as doing so.

**Copyrights**

IEEE draft and approved standards are copyrighted by IEEE under U.S. and international copyright laws. They are made available by IEEE and are adopted for a wide variety of both public and private uses. These include both use, by reference, in laws and regulations, and use in private self-regulation, standardization, and the promotion of engineering practices and methods. By making these documents available for use and adoption by public authorities and private users, IEEE does not waive any rights in copyright to the documents.

**Photocopies**

Subject to payment of the appropriate fee, IEEE will grant users a limited, non-exclusive license to photocopy portions of any individual standard for company or organizational internal use or individual, non-commercial use only.  To arrange for payment of licensing fees, please contact Copyright Clearance Center, Customer Service, 222 Rosewood Drive, Danvers, MA 01923 USA; +1 978 750 8400. Permission to photocopy portions of any individual standard for educational classroom use can also be obtained through the Copyright Clearance Center.

**Updating of IEEE Standards documents**

Users of IEEE Standards documents should be aware that these documents may be superseded at any time by the issuance of new editions or may be amended from time to time through the issuance of amendments, corrigenda, or errata. An official IEEE document at any point in time consists of the current edition of the document together with any amendments, corrigenda, or errata then in effect.

Every IEEE standard is subjected to review at least every ten years.  When a document is more than ten years old and has not undergone a revision process, it is reasonable to conclude that its contents, although still of some value, do not wholly reflect the present state of the art. Users are cautioned to check to determine that they have the latest edition of any IEEE standard.

In order to determine whether a given document is the current edition and whether it has been amended through the issuance of amendments, corrigenda, or errata, visit the IEEE-SA Website at <http://ieeexplore.ieee.org/xpl/standards.jsp> or contact IEEE at the address listed previously. For more information about the IEEE SA or IEEE’s standards development process, visit the IEEE-SA Website at <http://standards.ieee.org>.

**Errata**

[Errata](http://standards.ieee.org/findstds/errata/index.html), if any, for all IEEE standards can be accessed on the IEEE-SA Website at the following URL: <http://standards.ieee.org/findstds/errata/index.html>. Users are encouraged to check this URL for errata periodically.

**Patents**

Attention is called to the possibility that implementation of this standard may require use of subject matter covered by patent rights. By publication of this standard, no position is taken by the IEEE with respect to the existence or validity of any patent rights in connection therewith. If a patent holder or patent applicant has filed a statement of assurance via an Accepted Letter of Assurance, then the statement is listed on the IEEE-SA Website at <http://standards.ieee.org/about/sasb/patcom/patents.html>. Letters of Assurance may indicate whether the Submitter is willing or unwilling to grant licenses under patent rights without compensation or under reasonable rates, with reasonable terms and conditions that are demonstrably free of any unfair discrimination to applicants desiring to obtain such licenses.

Essential Patent Claims may exist for which a Letter of Assurance has not been received. The IEEE is not responsible for identifying Essential Patent Claims for which a license may be required, for conducting inquiries into the legal validity or scope of Patents Claims, or determining whether any licensing terms or conditions provided in connection with submission of a Letter of Assurance, if any, or in any licensing agreements are reasonable or non-discriminatory. Users of this standard are expressly advised that determination of the validity of any patent rights, and the risk of infringement of such rights, is entirely their own responsibility. Further information may be obtained from the IEEE Standards Association.

Participants

At the time this draft trial-use standard was completed, the Task Group TGaq of Working Group 11 had the following membership:

Stephen McCann, Chair

Yunsong Yang, Vice Chair

Participant1

Participant2

Participant3

Participant4

Participant5

Participant6

Participant7

Participant8

Participant9

The following members of the <individual/entity> balloting committee voted on this trial-use standard. Balloters may have voted for approval, disapproval, or abstention.

[To be supplied by IEEE]

Balloter1

Balloter2

Balloter3

Balloter4

Balloter5

Balloter6

Balloter7

Balloter8

Balloter9

When the IEEE-SA Standards Board approved this trial-use standard on <Date Approved>, it had the following membership:

[To be supplied by IEEE]

<Name>, Chair

<Name>, Vice Chair

<Name>, Past Chair

<Name>, Secretary

SBMember1

SBMember2

SBMember3

SBMember4

SBMember5

SBMember6

SBMember7

SBMember8

SBMember9

\*Member Emeritus

Also included are the following nonvoting IEEE-SA Standards Board liaisons:

<Name>, DOE Representative

<Name>, NIST Representative

<Name>

IEEE Standards Program Manager, Document Development

<Name>

IEEE Standards Program Manager, Technical Program Development

*{Editor’s note: The revision log table below shall be removed before publication}*

|  |
| --- |
| P802.11aq Draft Revision LogLast updated: 2014-09-30 |
| Editor: Dan Gal dan.gal@alcatel-lucent.com  |
|  |
| Revision Number | Date | Source Contributions  | Authors | Notes |
| 0.01 | 2014-06-04 | * 11-13-0299-03-00aq-draft-tgaq-terminology.docx
* 11-13-0300-01-00aq-proposed-specification-framework-for-tgaq.docx
* 11-14-0657-00-00aq-pre-association-discovery-protocol.doc
 | Various TGaq members | Initial TG draft |
| 0.02 | 2014-10-01 | * 11-14-0925-00-00aq-editorial-comments-on-d0-01.ppt
* 11-14-1277-02-00aq-simplification-of-service-identifiers.doc
 | Stephen McCann |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Introduction

This introduction is not part of P802.11aq/D0.02, Draft Trial-Use Standard for Information technology--Telecommunications and information exchange between systems Local and metropolitan area networks--Specific requirements Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications – Amendment: Pre-Association Discovery

.

This standard defines one medium access control (MAC) and several physical layer (PHY) specifications for wireless connectivity for fixed, portable, and moving stations (STAs) within a local area. It defines modifications to the IEEE 802.11 standard, above the physical layer (PHY), to enable delivery of pre-association Service Discovery information by IEEE 802.11 stations (STAs).

Contents

*<After draft body is complete, select this text and click Insert Special->Add (Table of) Contents>*

Draft Trial-Use Standard for Information technology--Telecommunications and information exchange between systems Local and metropolitan area networks--Specific requirements Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications – Amendment: Pre-Association Discovery

IMPORTANT NOTICE: IEEE Standards documents are not intended to ensure safety, security, health, or environmental protection, or ensure against interference with or from other devices or networks. Implementers of IEEE Standards documents are responsible for determining and complying with all appropriate safety, security, environmental, health, and interference protection practices and all applicable laws and regulations.

This IEEE document is made available for use subject to important notices and legal disclaimers.
These notices and disclaimers appear in all publications containing this document and may
be found under the heading “Important Notice” or “Important Notices and Disclaimers
Concerning IEEE Documents.” They can also be obtained on request from IEEE or viewed at <http://standards.ieee.org/IPR/disclaimers.html>.

1. Overview
	1. Scope
	2. Purpose
2. Normative references

The following referenced documents are indispensable for the application of this document (i.e., they must be understood and used, so each referenced document is cited in text and its relationship to this document is explained). For dated references, only the edition cited applies. For undated references, the latest edition of the referenced document (including any amendments or corrigenda) applies.

[1]. P802.11aq PAR: <https://development.standards.ieee.org/get-file/P802.11aq.pdf?t=77398700003>

 [2]. P802.11aq Use Cases: <https://mentor.ieee.org/802.11/dcn/12/11-12-1416-00-0pad-use-cases-and-requirements.doc>

[3]. P802.11aq Use Cases Analysis, Rev 6: <https://mentor.ieee.org/802.11/dcn/13/11-13-0125-06-00aq-use-case-analysis.doc>

[4]. IEEE Standards Definition Database online: http:// <http://dictionary.ieee.org/>

[5]. IEEE 802.11 [draft] standard: P802.11mc Rev: \_\_\_\_\_\_\_ Dated: \_\_\_\_\_\_\_\_\_\_

* 1. Definitions

For the purposes of this document, the following terms and definitions apply. The IEEE Standards Dictionary Online [4] should be consulted for terms which not defined in this clause. [[2]](#footnote-2)

**3GPP Access Network Discovery and Selection Function (ANDSF):** An entity within a 3GPP Evolved Packet Core (EPC) of the system architecture evolution (SAE), for 3GPP compliant mobile networks. The purpose of the ANDSF is to assist user equipment (UE) to discover non-3GPP access networks, such as WLAN, that can be used for data communications in addition to 3GPP access networks, such as HSPA or LTE, and to provide the UE with rules policing the connection to these networks.

**Application:** All the software that causes a device to perform a particular useful task beyond the running of the device itself.

**Bonjour:** A popular implementation of Zero configuration networking (Zeroconf), a group of technologies that includes service discovery, address assignment, and hostname resolution. Bonjour locates devices such as printers, other computers, and the services that those devices offer on a local network using multicast Domain Name System (mDNS) service records.

**Pre-Association Discovery Protocol (PADP):** A protocol to enable the discovery of service information for a pre-associated STA.

**Proximity:** Nearness in space, within the reception range of a radio frequency (RF) signal.

**Service:** An independently operable component of a peer unit that processes requests and associated data from clients in other peer units (peer services). Or an action or response initiated by a process (i.e., a server) at the request of some other process (i.e., a client) (peer and client services).

**Service Discovery:** The process of finding services that match the requirements of the service requestor. It includes procedures for querying and browsing for services offered by, or through, another STA.

**Service Discovery Protocols (SDPs**): Network protocols that allow automatic detection of STAs and services offered by these STAs on a computer/wireless network. Service discovery requires a common language to allow software agents to make use of one another's services without the need for continuous user intervention. Examples of service discovery protocols include Bluetooth Service Discovery Protocol (SDP), DNS Service Discovery (DNS-SD) as used in Bonjour, Dynamic Host Configuration Protocol (DHCP), Internet Storage Name Service (iSNS), Service Location Protocol (SLP), Simple Service Discovery Protocol (SSDP) as used in Universal Plug and Play (UPnP), Universal Description Discovery and Integration (UDDI) for web services, Web Proxy Autodiscovery Protocol (WPAD), WS-Discovery (Web Services Dynamic Discovery), and XMPP Service Discovery (XEP-0030).

**Universal Plug and Play (UPnP):** A set of networking protocols that permit networked devices, such as personal computers, printers, Internet gateways, access points and mobile devices to seamlessly discover each other's presence on the network and establish functional network services for data sharing, communications, and entertainment. The UPnP architecture is a distributed open networking architecture that leverages TCP/IP and the Web to enable seamless proximity networking in addition to control and data transfer among networked devices. UPnP technology is independent of any particular operating system, programming language, or network technology.

**Universally Unique Identifier (UUID):**is an identifier that is uniquely identifies a service

**Service Hash**: Hash value formed by using the first 6 octets of the SHA-256 algorithm hashing of the value of the service name or UUID.

**Upper Layer Protocol (ULP):** A protocol which operates at a higher OSI layer than the MAC layer of IEEE 802.11

* 1. Definitions specific to IEEE 802.11

----- {TBD} -----

* 1. Abbreviations and acronyms

ANDSF Access Network Discovery and Selection Function

App Application

SDP Service Discovery Protocol

SLP Service Location Protocol

SSDP Simple Service Discovery Protocol

UPnP Universal Plug and Play

1. { TBD?}

4.5.9 Interworking with external networks

*Change the text as follows*
{Editor note: need to show the changed text with Track Changes marks}

The interworking service allows non-AP STAs to access services provided by an external network according to the subscription or other characteristics of that external network. An IEEE 802.11 non-AP STA may have a subscription relationship with an external network, e.g., with an SSPN.

An overview of the interworking functions addressed in this standard is provided below:

— Network discovery and selection

— Discovery of suitable networks through the advertisement of access network type, roaming

consortium and venue information, via management frames

— Selection of a suitable IEEE 802.11 infrastructure using advertisement services (e.g., Access Network Query Protocol (ANQP) or an IEEE 802.21 Information Server) in the BSS or in an external network reachable via the BSS.

— Selection of an SSPN or external network with its corresponding IEEE 802.11 infrastructure

— Pre-Association Discovery

— Discovery of services offered by an infrastructure network in prior to association.

— Emergency services

— Emergency Call and Network Alert support at the link level

— QoS Map distribution

— SSPN interface service between the AP and the SSPN

{TBD – add the PAD element to the Beacon and Probe Response management frames}

**8.4.2.1 General**

*Insert the following row (ignoring the header row) in Table 8-1 after <preceding amendment last entry>*

|  |  |  |
| --- | --- | --- |
|  |  | Table 8-54 – Element IDs |
| Element | Element ID | Length of indicated element (in octets) | Extensible |
| Service Hint Information (see 8.4.2.122a) | <TBD> | <TBD> |  |
| Service Advertisement Information (see 8.4.2.122b) | <TBD> | <TBD> |  |
| Service Hash (see 8.4.2.122c) | <TBD> | <TBD> |  |
| Supported ULP (see 8.4.2.122d) | <TBD> | <TBD> |  |

**8.4.2.95 Advertisement Protocol element**

*Insert the following row (ignoring the header row) in Table 8-175 after Registered location query protocol (RLQP):*

|  |
| --- |
| Table 8-175 - Advertisement protocol ID definitions |
| Name | Value |
| Pre-Association Discovery Protocol | <ANA> |

*Insert dashed list text after Registered location query protocol (RLQP) as follows:*

—The Pre-association Discovery Protocol (PADP) supports service information retrieval. PADP is a protocol used by a requesting STA to query another STA (i.e., the receiving STA can respond to queries with and without proxying the query to a server in an external network). See 10.24 (WLAN interworking with external networks procedures) for information on PADP procedures.

*{Need some text to explain the two-stage process}*

*PADP consists of the following procedures:*

1. *Unsolicited PAD from an AP to a non-AP STA as described in 10.24.3.4.1*
2. *Solicited PAD from non-AP STA to an AP as described in 10.24.3.4.2*
3. *PADP request/response, typically from a non-AP STA to an AP for a more detailed service discovery query as described in 8.4.6.2.*

*Insert the following new subclause after <TBD> at the end of 8.4.2.*

**8.4.2.122a Service Hint Information element**

The Service Hint Information element contains information identifying services that are supported by an AP. The Service Information element is transmitted in beacons.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Element ID | Length | Bloom Filter Information | *m*-bit Service Hint Map |
| Octets | 1 | 2 | 2 | variable |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

Figure 8-401aq – Service Hint Information element format

The Element ID field and Length fields are defined in 8.4.2.1 (General). *{this table requires a new value added to it}.*

The value of the Length field is 2 plus the variable length *m*-bit Service Hint Map.

The Bloom filter information field is a 2-octet field representing the settings of the Bloom filter. The format of the Bloom filter information is shown in Figure 8-402aq.

|  |  |  |  |
| --- | --- | --- | --- |
|  | Number of services | Number of Hash functions | Reserved |
| Bit: | 0-8 | 9-12 | 13-15 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

Figure 8-402aq – Bloom filter information element format

The number of services field is used to indicate the maximum number of services, *n* that can be supported by the AP. The maximum number of services are 512

The number of Hash functions field is used to indicate the number of hash functions, *k* (out of maximum of 16) used by the Bloom filter. For example, 0001 means the first 2 Hash functions (denoted by Hash function index 0x00 and 0x01 as shown in Table 10-xyaq) are used.

**8.4.2.122b Service Advertisement Information (SAI) element**

The Service Advertisement Information (SAI) element identifies a service advertised by an AP.

The SAI element is included in the Probe Response by the AP, in response to a Probe Request from a non-AP STA that has one or more matching Service Hashes. For each matching Service Hash, the AP includes a corresponding Basic Service Descriptor.

The format of the SAI element is shown in Figure 8-403aq.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | One or more Basic Service Descriptors |
|  | Element ID | Length | Basic Service Information Descriptor |
| Octets | 1 | 1 | variable  |

**Figure 8-403aq – Service Advertisement Information element format**

The Element ID field and Length field are defined in 8.4.2.1 (General).

The format of the Basic Service Information Descriptor is shown in Figure 8-404aq.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Advertisement ID | Service Name Length | Service Name | ServiceStatus |
| Octets: | 4 | 1 | Variable | 1 |

**Figure 8-404aq – Basic Service Information Descriptor format**

The advertisement ID field is a 4-octet unsigned integer assigned by the AP when advertising a service.

The Service Name Length filed is the length of the Service Name field.

The Service Name field is an UTF-8 encoded string with maximum length of 64 bytes. It may be an official IANA registered name as defined in RFC 6335 or developer specified name.

The Service Status field is a 1octet field indicating the current status of the service as shown in Table 8-4xxaq.

**Table 8-4xxaq –Service Status value**

|  |  |
| --- | --- |
| Service Status Value | Description |
| 0 | Not available |
| 1 | Available |
| 2-255 | Reserved  |

**8.4.2.122c Service Hash element**

The Service Hash element consists of Service Hash Values. The Service Hash element may be included in the Probe Request frame.

The format of the Service Hash element is shown in Figure 8-405aq.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | One or more Service Hash Values |
|  | Element ID | Length | Service Hash Value |
| Octets | 1 | 1 | Multiple of 6 octets with each 6-octet representing a service  |

**Figure 8-405aq – Service Hash element format**

The Element ID field and Length fields are defined in 8.4.2.1 (General).

The Service Hash Value field contains one or more Service Hash Values. The Service Hash Value is formed from the value of service name by using the first 6 octets of the SHA-256 algorithm hashing of the value of the service name.

**8.4.2.122d Supported ULP Element**

The Supported ULP element is used to indicate the supported ULP by the AP. The Supported ULP may be included in the Beacon frame and Probe Response frame

The format of the Supported ULP element is shown in Table 8-40xaq:

|  |  |  |  |
| --- | --- | --- | --- |
|  | Element ID | Length | Supported ULP Bitmap  |
| Octets | 1 | 1 | 4 |

**Figure 8-40xaq – Supported ULP element format**

The Element ID field and Length fields are defined in 8.4.2.1 (General).

The Supported ULP Bitmap field is a 4-octets field that represents the set of supported ULPs by the AP.

**Table 8-402aq – Supported ULP Bitmap**

|  |  |  |
| --- | --- | --- |
| **ULP name** | **ULP Abbreviation** | **Bits** |
| DNS Service Discovery, part of Apple’s Bonjour technology | DNS-SD, Bonjour | 0 |
| Service Location Protocol | SLP | 1 |
| Simple Service Discovery Protocol as used in Universal Plug and Play | SSDP, UPnP | 2 |
| Universal Description Discovery and Integration for web services | UDDI | 3 |
| Jini for Java objects. | JINI | 4 |
| Bluetooth Service Discovery Protocol | SDP | 5 |
| Salutation | Salutation | 6 |
| XMPP Service Discovery | XEP-0030 | 7 |
| Web Services Dynamic Discovery | WS-Discovery | 8 |
| multicast DHCP | MDHCP | 9 |
| Internet Storage Name Service | iSNS | 10 |
| Web Proxy Autodiscovery Protocol | WPAD | 11 |
| Dynamic Host Configuration Protocol | DHCP | 12 |
| eXtensible Resource Descriptor Sequence | XRDS | 13 |
| e911 (Emergency Service) | e911 | 14 |
| Next Generation 911 (Emergency Service) | NG911 | 15 |
| Location Service | Location | 16 |
| Reserved  |  | 17-29 |
| Message Queue Telemetry Transport | MQTT | 30 |
| Vendor Specific |  | 31 |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

*Insert the following new subclause 8.4.6*

**8.4.6 Pre-Association Discovery Protocol elements**

**8.4.6.1 General**

PADP-elements are defined to have a common format consisting of a 2-octet Info ID field, a 2-octet Length field, and a variable-length element-specific Information field. Each element is assigned a unique Info ID as defined on this standard. The PADP-element format is shown in Figure 8-406aq:

|  |  |  |  |
| --- | --- | --- | --- |
|  | Info ID | Length | PADP Protocol-specific Information |
| Octets: | 2 | 2 | Variable |

**Figure 8-406aq – PADP-element format**

Each PADP-element in 8.4.6 is assigned a unique 2-octet Info ID .The set of valid Info IDs is defined in Table 8-xx1.

**Table 8-xx1 PADP-element definitions**

|  |  |  |
| --- | --- | --- |
| PADP-element name | Info ID | PADP-element (subclause) |
| Reserved | 0-275 |  |
| Service Information Request | 276 | 8.4.6.2 |
| Service Information Response | 277 | 8.4.6.3 |
| Encapsulation PADP | 278 | 8.4.6.3 |
| Reserved | 279- 65 535 | TBD |

The Length field is a 2-octet field that indicates the number of octets in the Information field and is encoded following the conventions given in 8.2.2 (Conventions).

The PADP Protocol-Specific Information field is a variable length field that contains a specific PADP element definition.

**8.4.6.2.Service Information Request PADP-element**

The Service Information Request element is used to request service information between STAs using the PADP Service Information Request/Response protocol. The Service Information Request element is included in a GAS Query Request and is sent by the non-AP STA to the AP.

The format of the Service Information Query Request is shown in Figure 8-407aq.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | Info ID | Length  | Service Name Length | Service Name | Service Information Query Request Length | Service Information Query Request |
| Octets: | 2 | 2 | 1 | variable | 1 | variable |

**Figure 8-407aq – Service Information Request PADP-element format**

The Service Information Query Request field contains service specific query such as key-value query.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |

**8.4.6.3 Service Information Response PADP-element**

The Service Information Response element is used to provide detailed service information between STAs using the GAS protocol in response to a Service Information Request element. The Service Information Response element is included in a GAS Query Response sent by the AP to the non-AP STA

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | One or more Detailed Service Information Descriptor |
|  | Info ID | Length | Detailed Service Information Descriptor |
| Octets | 2 | 2 | variable |

**Figure 8-408aq – Detailed Service Information Response PADP-element format**

The Service Information Descriptor field is a variable length field. The format of the Detailed Service Information Descriptor is shown in Figure 8-409aq

|  |  |  |
| --- | --- | --- |
| Basic Service Information Descriptor | Service Information Query Response Length | Service Information Query Response |
| variable  | 2 | variable |

**Figure 8-409aq – Detailed Service Information Descriptor element format**

The Service Information Query Response field is a variable length field. The format of the Service Information Query Response is service specific that contains requested service information

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

**8.4.6.4 Encapsulation PADP-element**

The Encapsulation element is used to exchange upper layer protocol (ULP) frames between STAs using the GAS protocol. The Encapsulation PADP-element is used as a transaction request included in a GAS Query Request or returned as a transaction response in the GAS Query Response.

|  |  |  |
| --- | --- | --- |
|  | Token | <TBD> |
| Octets: | 2 | variable |

**Figure 8-409aq – Encapsulation PADP-element format**

The Length and Token fields are defined in 8.4.6.1 (General).

The format of the <TBD> sub-field is <TBD>.

**10. MLME**

**10.24 WLAN interworking with external networks procedures**

**10.24.3 Interworking procedures: generic advertisement service (GAS)**

*Insert new subclause 10.24.3.4 after the end of 10.24.3.3 as follows:*

**10.24.3.4 Pre-Association Discovery Protocol (PADP) procedures**

**10.24.3.4.1 General**

PADP provides functionality that enables STAs to discover the availability of services offered by an AP, before they associate with the wireless LAN. While the specification of service specific information is outside the scope of this standard, the AP can act as a proxy to the services offered by an external network or services offered by non-AP STAs associated with the AP.

There are two types of PAD namely unsolicited and solicited.

In the unsolicited PAD, basic service information is included in the Beacons, transmitted by the AP. Upon receiving the Beacons frames, the non-AP STAs can make an informed decision to associate with the AP, or query for more detailed service information using PADP as described in 8.4.6.2 before association.

In the solicited PAD, basic service information is included in the Probe Request transmitted by the non-AP STA. Upon receiving the Probe Request, the AP responds with a Probe Response only if there is a service match between the non-AP STA and the AP. The non-AP STAs can make an informed decision to associate with the AP or query for more detailed service information using PADP as described in 8.4.6.2 before association

**10.24.3.4.1 Unsolicited PAD**

An AP having dot11UnsolictedPADActivated equals to true shall include a Service Hint Information element or Service Advertisement Information element or both in Beacon frames.

The non-AP STA may associate to the AP based on the received Service Hint Information element or may use PADP Service Information Request to request more detailed information as defined in Table 8-175 (Advertisement protocol ID definitions) prior to association. The receiving AP shall respond to the PADP Service Information Request with PADP Service Information Response.

**10.24.3.4.2 Solicited PAD**

A non-AP STA having dot11PADActivated equals to true may send Probe Request containing Service Hash element

An AP having dot11SolictedPADActivated equals to true shall include Service Advertisement Information element in Probe Response frame, if there is one or more Service Hashes matching with the received Probe Request containing the Service Hash element sent by the non-AP STA.

The non-AP STA may associate to the AP based on the received Service Advertisement Information element or may use PADP Service Information Request to request more detailed information as defined in Table 8-175 (Advertisement protocol ID definitions) prior to association. The receiving AP shall respond to the PADP Service Information Request with PADP Service Information Response.

A STA that encounters an unknown or reserved PADP Info ID value in a GAS frame (see 8-210) received without error shall ignore that PADP Info ID and shall parse any remaining PADP Info IDs.

A STA that encounters an unknown vendor-specific PADP-element field or subfield in a GAS frame (see 8-210) received without error shall ignore that field or subfield respectively, and shall parse any remaining fields or subfields for additional information with recognizable field or subfield values.

**10.24.3.4 PAD Encapsulation Protocol procedures**

<TBD> - Normative description of the protocol here.

**10.x.x Hash Function for Bloom Filter Operation**

The Bloom filter Hash function is as follows. Each Service Hash is hashed to *j* bit positions in the *m*-bit Service hint map using *j* hash functions. A total of 16 Hash functions are defined and are constructed as follows:

Let H(*j*,X,*m*) denotes the Hash function with

1. *j* Bloom filter Hash Function pre-pend parameter used in the computation. *j* ranges from 0x00, 0x0F in hexadecimal notation.
2. X is the Service Hash that is mapped to *j*-bits of the *m*-bits Service Hint Map
3. *m* is the size of Bloom filter to be indicated in bits

*H*(*j*,X,*m*) is computed as follows:

1. Compute A(*j*,X) = [*j* || X] where || denotes an append operation
2. Compute B(*j*,X) = CRC32(A(*j*,X)) & 0x0000FFFF. i.e., obtain the last 2 bytes 32 bit CRC of A(*j*,X) where the CRC operation is seeded with 0xFFFFFFFF.
3. H(*j*,X,*m*) = B(*j*,X) mod *m*

The full set of Hash functions is shown in Table 8-xyaq.

|  |  |
| --- | --- |
| Hash Function Index, *j* (in Hexadecimal)  | Hash Function  |
| 0x00 | H(0x00,X,*m*) |
| 0x01 | H(0x01,X,*m*) |
| 0x02 | H(0x02,X,*m*) |
| 0x03 | H(0x03,X,*m*) |
| 0x04 | H(0x04,X,*m*) |
| 0x05 | H(0x05,X,*m*) |
| 0x06 | H(0x06,X,*m*) |
| 0x07 | H(0x07,X,*m*) |
| 0x08 | H(0x08,X,*m*) |
| 0x09 | H(0x09,X,*m*) |
| 0x0A | H(0x0A,X,*m*) |
| 0x0B | H(0x0B,X,*m*) |
| 0x0C | H(0x0C,X,*m*) |
| 0x0D | H(0x0D,X,*m*) |
| 0x0E | H(0x0E,X,*m*) |
| 0x0F | H(0x0F,X,*m*) |

Table 10-xyaq – Hash functions for the Bloom filter

**Annex C**

**(normative)**

**ASN.1 encoding of the MAC and PHY MIB**

**C.3 MIB Detail**

***Insert new MIB values as follows:***

dot11PADImplemented OBJECT-TYPE

 SYNTAX TruthValue

 MAX-ACCESS read-only

 STATUS current

 DESCRIPTION

"This is a capability variable. Its value is determined by device capabilities.

This attribute when true, indicates the STA is capable of pre-association discovery (PAD)

with external networks. A STA setting this to true implements PAD. When this is false, the STA

 does not implement PAD.

 DEFVAL {false}

::= { dot11StationConfigEntry *<TBD>*}

dot11PADActivated OBJECT-TYPE

 SYNTAX TruthValue

 MAX-ACCESS read-write

 STATUS current

 DESCRIPTION

 "This is a control variable.

It is written by an external management entity or the SME. Changes take

 effect as soon as practical in the implementation.

This attribute when true, indicates the capability of the STA to operate PAD

with external networks is enabled. The capability is disabled otherwise."

 DEFVAL {false}

::= { dot11StationConfigEntry *<TBD>*}

**Annex AQ1**

**(normative)**

**AQ1.1 Service Discovery**



.

**Annex AQ2**

**(normative)**

**AQ2.1 Proxy Entity**

{<placeholder> for description of a service directory in the STA}. This is required to pass information up to higher layer applications (e.g. a Service Hash) and for the PADP to work.

It is assumed that there is proxy function in the network that maintains a list of services. The upper layer protocols are not exposed to un-associated STAs. The proxy is used to encapsulate the service identifiers and exchange that information to the STA. Therefore, PADP is opaque to the service definition and is handled by the proxy and the end STA itself.

# (Informative)Bibliography

Bibliographical references are resources that provide additional or helpful material but do not need to be understood or used to implement this standard. Reference to these resources is made for informational use only.

Annex (How m is determined or calculated)

Annex (Deployment Guidelines)

1. The Institute of Electrical and Electronics Engineers, Inc.

3 Park Avenue, New York, NY 10016-5997, USA

Copyright © 2014 by The Institute of Electrical and Electronics Engineers, Inc.

All rights reserved. Published <Date Published>. Printed in the United States of America.

IEEE is a registered trademark in the U.S. Patent & Trademark Office, owned by The Institute of Electrical and Electronics
Engineers, Incorporated.

PDF: ISBN 978-0-XXXX-XXXX-XSTDXXXXX

Print: ISBN978-0-XXXX-XXXX-XSTDPDXXXXX

IEEE prohibits discrimination, harassment, and bullying.

For more information, visit <http://www.ieee.org/web/aboutus/whatis/policies/p9-26.html>.

No part of this publication may be reproduced in any form, in an electronic retrieval system or otherwise, without the prior written permission of the publisher. [↑](#footnote-ref-1)
2. IEEE Standards Dictionary Online subscription is available at:

<http://www.ieee.org/portal/innovate/products/standard/standards_dictionary.html>. [↑](#footnote-ref-2)