IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Changes for 4.5.4 |
| Date: 2020-08-18 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Hitoshi Morioka | SRC Software | Fukuoka, JAPAN |  | hmorioka@src-soft.com |
|  |  |  |  |  |

Abstract

This document describes proposed changes for clause 4.5.4 in D0.1.

4.5.4 Access control and data confidentiality services

*~~Change the nth paragraphs as follows:~~*

~~The current IEEE Std. 802.11 has a group temporal key security association (GTKSA) security framework for multicast that does not protect origin authenticity between devices having that GTKSA. Such protection is needed in some broadcast use cases.~~

4.5.4.6 Data origin authenticity

*Change the second paragraph as follows:*

Data origin authenticity is applicable only to individually addressed Data frames, and individually addressed robust Management frames on non-eBCS STAs. ~~The protocols do not guarantee data origin authenticity for group addressed frames, as this cannot be accomplished using symmetric keys and public key methods are too computationally expensive.~~ The enhanced broadcast service (eBCS) provides data origin authenticity for group addressed frames.