### **IEEE P802.11 Wireless LANs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB266 CR for 9.3.1.22.3 | | | | |
| Date: 2022-07-07 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Yanjun Sun | Qualcomm |  |  |  |
| Steve Shellhammer |  |  |  |  |
| Alfred Asterjadhi |  |  |  |  |
| George Cherian |  |  |  |  |
| Abhishek Patil |  |  |  |  |
| Youhan Kim |  |  |  |  |
| Bin Tian |  |  |  |  |
| Duncan Ho |  |  |  |  |
| Gaurang Naik |  |  |  |  |
| Abdel Karim Ajami |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Abstract**

This submission proposes resolutions for the following CIDs for TGbe LB266: 12345 and 10375

**Revisions:**

* Rev 0: Initial version of the document.

***TGbe editor: Please note Baseline is IEEE 802.11-2020, 11ax D8.0, and 11be D2.0***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CID | Commenter | Clause | Page | Comment | Proposed Change | Resolution |
| 12345 | John Coffey | 9.3.1.22.3 | 152.29 | Singular/plural discrepancy: "except [X] and [Y], which is defined" | Change "is" to "are" | Accepted  Tgbe editor please implement changes proposed by the Commenter. |
| 10375 | Mengshi Hu | 9.3.1.22.3 | 153.04 | It is a little bit confusing that AID12 subfield = 4095 is disallowed in a User Info field, but the table shows the AID12 subfield encoding in the User Info field for 4095. If 4095 is not allowed, suggest removing the row 4095 and move those descriptions to the NOTE of the table. | Remove the row 4095 and move those descriptions to the NOTE of the table. | Revised  Agree with the commenter in principle. The row has been deleted and NOTE is revised as suggested.  Tgbe editor please implement changes as shown in doc 11-22/0993r0 tagged as #10375 |

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

**9.3.1.22.3 HE variant User Info field**

***TGbe editor: Please delete the row with 4095 in the first column and update the NOTE (Starting from P153L3 in D2.0) as follows (track change enabled):***

**Table 9-51—AID12 subfield encoding**

|  |  |
| --- | --- |
| **AID12 subfield** | **Description** |
| 0 | User Info field allocates one or more contiguous RA-RUs for associated STAs |
| 1–2007 | User Info field is addressed to an associated STA whose AID is equal to the value in the AID12 subfield |
| 2008–2044 | Reserved |
| 2045 | User Info field allocates one or more contiguous RA-RUs for unassociated STAs |
| 2046 | Unallocated RU |
| 2047–4094 | Reserved |

**Table 9-51—AID12 subfield encoding *(continued)***

|  |  |
| --- | --- |
| (#10375) |  |
| NOTE—The Padding field, if present in a Trigger frame, is a field with all padding bits set to 1. The Padding field, if present, has a length of at least two octets and is located between the User Info List field and the FCS field. An AP does not set the AID12 subfield in a User Info field to 4095.(#10375) | |