EEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11be lb266 CR for clause 36.3.14 Packet Extension | | | | |
| Date: 2022-07-11 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Yan Zhang | NXP | 350 Holger Way, San Jose, CA, |  | [yan.zhang\_5@nxp.com](mailto:yan.zhang_5@nxp.com) |

Abstract: This document contains proposed resolutions for comments in *Clauses 36.3.14* from 11be D2.0 with 6 CID below

|  |  |  |
| --- | --- | --- |
| ***Clause 36.3.14***  10840, 11297, 12028, 12151, 12207, 12297 |  | |
|  | |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 10840 | 36.3.14 | 730.52 | The number of spatial streams larger than eight is not defined in the EHT. So, this sentence should be deleted. | Delete the text in P730L52. | **Accepted.**  Agree with commentor that the text is not needed since the maximum number of spatial streams is defined as 8 in 11be spec.  TGbe editor: Please delete the text on P730L52 as in comment. |
| 11297 | 36.3.14 | 730.52 | "an EHT MU PPDU with more than eight spatial streams transmitted on at least one RU or MRU". I believe this is not possible in R1. Why mention it? | remove bullet item | **Revised.**  Agree with commentor that the text is not needed since the maximum number of spatial streams is defined as 8 in 11be spec.  TGbe editor: Same resolution as CID 10840. |
| 12028 | 36.3.14 | 730.52 | 11be does not allow spatial streams more than 8. | Delete the condition "an EHT MU PPDU more than eight spatial streams transmitted on at least on RU or MRU". | **Accepted.**  Agree with commentor that the text is not needed since the maximum number of spatial streams is defined as 8 in 11be spec.  TGbe editor: Same resolution as CID 10840. |
| 12151 | 36.3.14 | 730.52 | In EHT PHY, the total spatial streams across all users not exceeding eight. The description "A PE field of duration 20 us is only allowed in the following cases: an EHT MU PPDU with more than eight spatial streams transmitted on at least one RU or MRU" is unnecessary. There is a similar issue on the sentence "more than eight spatial streams"at P525L14 and L29 (35.14.5). | At P730L52, remove "an EHT MU PPDU with more than eight spatial streams transmitted on at least one RU or MRU".  At P525L14, remove "or more than eight spatial streams are transmitted on the RU or MRU,".  At P525L29, remove ", or the RU or MRU uses more than eight spatial streamsr MRU". | **Accepted.**  Agree with commentor that the text is not needed since the maximum number of spatial streams is defined as 8 in 11be spec.  TGbe editor: Please delete the text on P525L14 “or more than eight spatial streams are transmitted on the RU or MRU,” and P525L29 “, or the RU or MRU uses more than eight spatial streamsr MRU”. |
| 12207 | 36.3.14 | 730.52 | Since the spec supports only up to 8 streams, why do we need to specify that one of the rules for PE duration to be 20usec is 'more than eight spatial streams'? | As long as no more than 8 spatial streams are defined, remove this sentence, and make similar changes below Table 9-401 and corresponding text in 35.14.5. | **Revised.**  Agree with commentor that the text is not needed since the maximum number of spatial streams is defined as 8 in 11be spec.  TGbe editor: Same resolution as CID 12151. |
| 12297 | 36.3.14 | 730.52 | It doesn't make sense to use a limitation based on more than 8 streams, when the max number of streams defined in the spec is 8. | It doesn't make sense to use a limitation based on more than 8 streams, when the max number of streams defined in the spec is 8. | **Accepted.**  Agree with commentor that the text is not needed since the maximum number of spatial streams is defined as 8 in 11be spec.  TGbe editor: Same resolution as CID 10840. |