IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB276 CR for CID 3338 | | | | |
| Date: 2023-11-14 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Dong Wei | NXP |  |  | dong.wei@nxp.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document aims to resolve the following LB276 comment: CID 3338.

R0: Initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 3338 | 9.3.1.22.14.6 | 41.09 | Not clear what the Partial TSF field contains if the AP did not transmit a Sensing Poll Trigger frame preceding the SR2SR Sounding Trigger frame. | Remove condition "if the AP transmitted the Sensing Polling Trigger frame that preceded the SR2SR Sounding Trigger frame carrying this User Info field.", or define contents of the Partial TSF field when no preceding Sensing Polling Trigger. | Revised  Incorporate the changes in  <https://mentor.ieee.org/802.11/dcn/23/11-23-2070-00-00bf-lb276-cr-for-cid-3338.docx> |

**Discussion:**

Since this CID is closely related to CIDs 3294 and 3337, the resolution for this CID should be consistent with the resolution for CIDs 3294 and 3337 (see document 23/1879).

*TGbf Editor: Please insert the following paragraph at the end of Clause 9.3.1.22.14.6 (SR2SR Sounding Trigger frame) of D2.1.*

Note - If there is no transmission of the Sensing Polling Trigger frame, the Partial TSF field and the Token filed in the User Info field with the AID12/USID12 subfield equal to 2008 is reserved.

**SP:** Do you agree to the resolution provided in the document 11-23/2070r0for CID 3338?