**IEEE P802.11  
Wireless LANs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB271 CR for CID 18025 | | | | |
| **Date**: July 11, 2023 | | | | |
| **Author(s):** | | | | |
| **Name** | **Affiliation** | **Address** | **Phone** | **email** |
| Yan Li | ZTE |  |  | li.yan16@zte.com.cn |
| Ke Tang |  |  |  |
| Zisheng Wang |  |  |  |
| Qisheng Huang |  |  |  |

**Abstract**

This submission proposes resolutions for following **1** CID received for TGbe LB271:

18025

**Revisions:**

* Rev 0: Initial version of the document.

***TGbe editor: The baseline for this document is P802.11beD3.0***

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e., they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Pg/Ln** | **Comment** | **Proposed Change** | **Resolution** |
| 18025 | Joseph Levy | 6.3.136.2.2 | 127/31 | The Delete Timer parameter can not contain the number of TBTTs of the affiliated AP until the affiliated AP is removed. The act of removal is an action of the non-AP MLD removing the affiliated AP from the MLD. It is not the act of the AP MLD of no longer supporting MLO over the affiliated AP. The AP only knows when the AP MLD will no longer support MLO on that AP. Therefore, the timer should provide the time when the AP MLD will no longer support MLO on the target affiliated AP. | Replace: "Specifies the number of TBTTs of the affiliated AP until the AP is removed."  With: "Specifies the number of TBTTs of the affiliated AP until the affiliated AP stops supporting MLO." | **Rejected.**  Firstly the action of removal is really the operation of AP MLD removing the affiliated AP,which finally refers to the corresponding BSS to be terminated.  Secondly it is odd to say affiliated AP supports MLO.The group has adopted removing affiliated AP terminology for many drafts and it is well understood what it means. Hence, no change is needed |